[bookmark: OLE_LINK146][image: MCj03463170000[1]]Safety Instruction
1. [bookmark: OLE_LINK149]Users are required to read the operation manual completely and carefully before installation or operation.
2. [bookmark: OLE_LINK152][bookmark: OLE_LINK153]The product should be installed and pre-operated by well-trained persons. All power supplies must be turned off during the installation work, remember not to operate with power on. 
3. All the instruction marked with sign [image: MCj03463170000[1]] must be observed or executed; otherwise, bodily injuries might occur.
4. [bookmark: OLE_LINK154][bookmark: OLE_LINK155]For perfect operation and safety, it is prohibited that using extension cable with multi-outlet for power connection. 
5. [bookmark: OLE_LINK156]When connecting the power cord, it must be determined that the operating voltage conforms to the rated voltage value specified in the product identification.
6. [bookmark: OLE_LINK166]Don’t operate in direct sun light，outdoors area and where the room temperature is over 45°C or below 0°C.
7. [bookmark: OLE_LINK167][bookmark: OLE_LINK168]Please avoid operating near the heater at dew area or at the humidity below 10% or above 90%.
8. [bookmark: OLE_LINK169]Don’t operate in area with heavy dust, corrosive substance or volatile gas.
9. [bookmark: OLE_LINK170][bookmark: OLE_LINK171]Avoid power cord being applied by heavy objects or excessive force, or over bend.
10. [bookmark: OLE_LINK172][bookmark: OLE_LINK173]The earth wire of power cord must be connected to the system ground of the production plant by proper size of conductions and terminals. This connection should be fixed permanently.
11. [bookmark: OLE_LINK174][bookmark: OLE_LINK175]All the moving portions must be prevented to be exposed by the parts provided.
12. [bookmark: OLE_LINK176]Turing on the machine in the first time, operate the sewing machine at low speed and check the correct rotation direction.
13. [bookmark: OLE_LINK177][bookmark: OLE_LINK178]Turn off the power before the following operation: 
[bookmark: OLE_LINK179][bookmark: OLE_LINK180]1. Connecting or disconnecting any connectors on the control box or motor.
[bookmark: OLE_LINK181][bookmark: OLE_LINK182]2. Threading needle.
[bookmark: OLE_LINK183][bookmark: OLE_LINK184]3. Raising the machine head.
[bookmark: OLE_LINK185][bookmark: OLE_LINK186]4. Repairing or doing any mechanical adjustment.
[bookmark: OLE_LINK187][bookmark: OLE_LINK188]5. Machines idling.
14. [bookmark: OLE_LINK189]Repairs and high level maintenance work should only be carried out by electronic technicians with appropriate training.
15. [bookmark: OLE_LINK190][bookmark: OLE_LINK191]All the spare parts for repair must be provided or approved by the manufacturer.
16. [bookmark: OLE_LINK192][bookmark: OLE_LINK193]Don’t use any objects or force to hit or ram the product.
Guarantee time
Warranty period of this product is 1 year dated from purchasing, or within 2 years from ex-factory date.
Warranty detail
Any trouble found within warranty period under normal operation, it will be repaired free of charge. However, maintenance cost will be charged in the following cases even if within warranty period:
[bookmark: OLE_LINK102][bookmark: OLE_LINK103]1. Inappropriate use, including: wrong connecting high voltage, wrong application, disassemble, repair, modification by incompetent personnel, or operation without the precaution, or operation out of its specification range, or inserting other objects or liquids into the product.
2. Damage by fire, earthquake, lighting, wind, flood, salt corrosive, moisture, abnormal power voltage and any other damage cause by the natural disaster or by the inappropriate environments.
3. Dropping after purchasing or damage in transportation by customer himself or by customer’s shipping agency
* We make our best effort to test and manufacture the product for assuring the quality. However, it is possible that this product can be damaged due to external magnetic interference and electronic static or noise or unstable power source more than expected; therefore the grounding system of operate area must guarantee the good earth and it’s also recommended to install a failsafe device (Such as residual current breaker).



1. Operation panel key function description
	No.
	Icon
	Name
	Function description

	1
	[image: ]
	Function key
	①In the normal mode interface, press it to enter the "User parameter setting" interface.
②Long press to turn on the machine and enter the "Technician parameter setting" interface.
③In the parameter setting interface, press it to return without saving the parameters.

	2
	[image: ]
	Save key
	In the parameter setting interface, press it to save.

	3
	[image: ]
	[bookmark: OLE_LINK3]Parameter increases / Speed increases
	①In the normal mode, press it can increase speed, long-press to increase speed quickly.
②In the parameter setting interface, press it can increase the parameter.

	4
	[image: ]
	Parameter decreases / Speed decreases
	①In the normal mode, press it can decrease speed, long-press to decrease speed quickly.
②In the parameter setting interface, press it can decrease the parameter.

	5
	[image: ]
	Left key / Cloth choice
	①In the parameter setting interface, press it can move the position of the parameter item to the left.
②In the normal mode interface, long-press it to enter the cloth choice mode.

	6
	[image: ]
	Right key / LED
	①In the parameter setting interface, press it can move the position of the parameter item to the right.
②In the normal mode interface, long-press it to enter the LED light brightness adjustment mode

	7
	[image: ]
	Front trimming / Back trimming
	①In the normal mode interface, press it can execute the cycle shift of front trimming on and front trimming off. Press up and down key can adjustment front trimming action time. (same as P-27)
②In the normal mode interface, long-press it can execute the cycle shift of back trimming on and back trimming off. Press up and down key can adjustment back trimming action time. (same as P-28)

	8
	[image: ]
	Mode selection /  Auto-suction mode
	①In the normal mode, press it can execute the cycle shift of the following four modes:
1. Full manual: start-up according to the pedal completion.
2. Free sewing.
3. Semi-automatic: start-up according to front sensor signal + pedal completion (same as P-05).
4. Automatic: start-up according to sensor signal.
②In the normal mode interface, long-press it can execute the cycle shift of suction off, front suction on, back suction on and suction on.

	9
	[image: ]
	Presser foot lifting / Sensor key
	①In the normal mode interface, press it can execute the cycle shift of function off, front presser foot lifting on, back presser foot lifting on and function on (same as P-10).
②In the normal mode interface, long-press it can check sensor real-time sensor value and current threshold value.

	10
	[image: ]
	Feed dog height / Stepping motor
	①In the normal mode interface, press it can execute the cycle shift of thin fabric, medium thick fabric, thick fabric.
②In the normal mode interface, long-press to enter the mode parameter and presser foot micro-lifting adjustment interface.

	11
	[image: ]
	Press foot height / Pedal gear
	①In the normal mode interface, press it can enter the presser foot height adjustment interface.
②In the normal mode interface, long-press to enter the pedal acceleration slope adjustment parameter.

	12
	[image: ]
	Switching
	In the normal mode interface, press it can execute the cycle shift of knitted T-shirt, denim, jacket and pants, elastic fabric and non-woven fabric modes.



2. Special function operation definition
	No.
	Function name
	Function description

	1
	Reset
	After powering on, press and hold [image: ] + [image: ] at the same time to restore factory settings.

	2
	Machine debugging interface
	After powering on, press and hold the [image: ] + [image: ] key at the same time to enter machine debugging interface.

	3
	Cloth identification mode
	Step 1: Long-press [image: ] key in the normal mode interface to enter cloth identification mode, making sure the sensor is not obstructed;
Step 2: Press [image: ] key to confirm, enter the cloth identification mode selection, and then press [image: ] key to confirm;
Step 3: Wait a few seconds, after jumping out of the cloth identification success interface, the cloth identification is successful.

	4
	Presser foot height adjustment
	Step 1: Press [image: ] key in the normal mode interface to enter presser foot height adjustment interface;
Step 2: Press [image: ] and [image: ] key to adjust presser foot height;
Step 3: Press [image: ] key after adjustment and the setting is completed.

	5
	Pedal sensitivity adjustment
	Step 1: Long-press [image: ] key in the normal mode interface to enter pedal sensitivity adjustment interface;
Step 2: Press [image: ] and [image: ] key to adjust sensitivity (slow speed, medium speed, fast, super-fast, top speed);
Step 3: Press [image: ] key after adjustment and the setting is completed.

	6
	Feed dog height adjustment
	In the normal mode interface, press [image: ] key to enter feed dog height adjustment interface, and then press [image: ] key to switch the corresponding to feed dog height (thin fabric, medium thick fabric, and thick fabric).

	7
	Piece counting function
	In the normal mode interface, press the [image: ] + [image: ] key to enter the piece counting interface.

	8
	Advanced parameter mode
	After powering on, press and hold [image: ] + [image: ] key at the same time, and enter the password to enter the advanced parameter mode interface.



3. System parameter setting definition
	User parameter (press [P] key to enter in normal mode)

	No
	Function parameters
	Range
	Default
	Description

	P-01
	[bookmark: OLE_LINK63][bookmark: OLE_LINK64][bookmark: OLE_LINK295][bookmark: OLE_LINK294]Sewing speed (r/min)
	200-7000
	6000
	

	P-02
	Needle stop positioning selection
	0-1
	0
	0: Upper needle position
1: Lower needle position

	P-03
	Trimming speed (r/min)
	200-7000
	5000
	With trimming function: the speed setting for front sensor trigger start-up and back sensor signal finish (before trimming).

	P-04
	Start-up mode
	0-1
	1
	(Valid for full-automatic mode)
0: Automatic mode
1: Foot control mode (start-up by front sensor + front pedal)

	P-05
	Automatic / semi-automatic 
mode selection
	0-1
	0
	(P-06 is turn on)
0: Automatic (match with P-04 use)
1: Semi-automatic (foot control mode)

	P-06
	Auto sensing switch
	0-1
	1
	0: OFF (full manual mode is turn on)   
1: ON (it can execute automatic / semi-automatic mode also match with P-05 use)

	P-07
	Auto trimming switch
	0-3
	3
	(P-70= Horizontal knife type, this parameter is valid)
0: OFF
1: Front trimming (trimming when Mid-sensor receive signal)
2: Back trimming (trimming after back-sensor receive signal) 
3: Front and back trimming

	
	Automatic thread tension releasing switch
	0-3
	2
	(P-70=side knife type, this parameter is valid)
0: OFF
1: Front thread tension releasing
2: Back thread tension releasing
3: Front and back thread tension releasing

	P-08
	Auto suction
	0-3
	0
	0: OFF
1: Front trimming suction
2: Back trimming suction 
3: Front and back trimming suction

	P-09
	Automatic cloth feeding
	0-1
	0
	(P-70= horizontal knife type, this parameter is valid)
0: OFF
1: Cloth feeding when sewing

	P-10
	Auto presser foot lifting
	0-3
	0
	0: OFF
1: Front presser foot lifting (when front sensor receive signal) 
2: Back presser foot lifting (after back sensor receive signal)
3: Front and back presser foot lifting

	P-11
	Presser foot lifting when stop on the sewing
	0-1
	0
	(Valid for full-manual and semi-automatic mode)
0: OFF
1: ON (when stop on the sewing the presser foot lifting automatically)

	P-12
	Presser foot lifting after trimming
	0-1
	0
	0: OFF
1: ON

	P-13
	Presser foot lifting when half back pedal
	0-2
	0
	(Valid for full-manual / semi-automatic mode)
0: Half back & full back
1: OFF
2: Full back

	P-14
	Manual suction
	0-2
	0
	0: OFF
1: Back suction
2: Front and back suction

	P-15
	Machine lamp brightness
	0-4
	3
	0: OFF
1→4: The brightness grade, the more value the more brightness.

	P-16
	Low air pressure mode
	0-1
	0
	0: Normal mode
1: Low pressure mode

	P-17
	Semi-automatic continuous sewing
	0-1
	0
	0: OFF
1: Front step continuous sewing
(P70=Horizontal knife model, default: 1; P70=Side knife model, default: 0)

	P-18
	Constant speed of thread trimming switch
	0-1
	0
	0: OFF (after finish before trimming not execute P-03 speed)
1: Constant trimming speed (The speed of front and back trimming is fixed to the speed of P-03)

	P-19
	Suction when back pedal
	0-2000
	0
	0: OFF
1-2000: suction holding time (ms)

	P-20
	Stop position selection after trimming
	0-1
	1
	0: Lower needle position
1: Upper needle position

	P-22
	Front receiver E# switch
	0-1
	1
	0: ON (turn on front sensor, sensor signal + pedal activated)
1: OFF (turn off front sensor, pedal directly activated)
(P70=Horizontal knife model, default: 0; P70=Side knife model, default: 1)

	P-23
	Intermittent suction opening time (×100ms)
	1-600
	20
	The more value the more time.

	P-24
	Intermittent suction stopping time (×100ms)
	0-600
	0
	0: For no intermittent air suction
Front suction off time (valid when P-46 function setting is 1).

	P-25
	Synchronous suction (P16=1)（ms）
	0-2000
	200
	Synchronous suction time of cloth (valid for P-16 setting is 1).

	P-26
	The stitches number between two sensors
	1-600
	100
	Cycle period parameter: In a circle the back sensor receive signal then can continue running, otherwise a cycle stop.

	P-27
	The delayed stitches number of front trimming (stitches)
	0-50
	3
	(P-70= Horizontal knife type, this parameter is valid)
The smaller the value, the earlier the advance, and the longer the thread residue (Mid-sensor trigger).

	P-28
	The delayed stitches number of back trimming (stitches)
	0-50
	3
	(P-70= Horizontal knife type, this parameter is valid)
The smaller the value, the earlier the advance, and the shorter the thread residue (Back-sensor trigger).

	
	The starting time for back thread tension releasing (stitches)
	0-50
	8
	(P-70= Side knife type, this parameter is valid)

	P-30
	The delayed time of front suction off (ms)
	100-5000
	100
	(P-70= Horizontal knife type, this parameter is valid)
The small value the close is fast.

	
	The stitches number when
front suction off (stitches)
	0-50
	15
	(P-70= Side knife type, this parameter is valid)

	P-31
	The delayed time of back suction off (ms)
	100-5000
	200
	The small value the close is fast.
(P70=Horizontal knife model, default: 300; P70=Side knife model, default: 1000)

	Technician parameter (hold [P] key to enter)

	P-35
	The delayed stitches number before the machine stops (stitches)
	1-99
	1
	After cloth has passed the sensor, the number of stitches when machine stop automatically. (Valid for back trimming off condition)
(P70=Horizontal knife model, default: 1; P70=Side knife model, default: 3)

	P-36
	The response time of front sensor (ms)
	10-990
	50
	The small value the response is fast, the large value the response is slow

	P-37
	The sensitivity of front sensor
	0-700
	300
	In order to adapt different cloth material setting front sensor receive strength.

	P-38
	The sensitivity of middle sensor
	0-700
	215
	In order to adapt different cloth material setting mid-sensor receive strength.

	P-39
	The holding time of front presser foot lifting (ms)
	10-2000
	200
	(In full automatic / semi-automatic mode)
[bookmark: OLE_LINK98][bookmark: OLE_LINK99]The larger value the longer holding time.

	P-40
	Back presser foot lifting start time (ms)
	0-2000
	120
	The starting time of back presser foot lifting, the smaller value the faster the response.

	P-41
	Full-on output time setting of presser foot (ms)
	10-990
	100
	The larger value the higher of foot lifting (noted: not too high)

	P-42
	Periodic signal of presser foot output (%)
	10-90
	25
	When the presser foot is moving, the output is periodically power-saved to prevent the electromagnet from getting hot

	P-43
	The time for the presser foot laying down (ms)
	10-990
	100
	The action time of presser foot laying down sequence.

	P-44
	Presser foot protection (s)
	1-120
	10
	Stop on the sewing the presser foot lifting, stop after trimming presser foot lifting, positive closing after heeling pedal for retention time.

	P-45
	Trimming time (ms)
	10-990
	30
	(P-70= Horizontal knife type, this parameter is valid)
the longer time, the greater trimming force

	
	[bookmark: _GoBack]Thread tension release time (ms)
	0-5000
	300
	(P-70= Side knife type, this parameter is valid)

	P-46
	Suction when continuous feeding
	0-2
	0
	0: No suction
1: Long suction
2: Synchronous suction
(P70=Horizontal knife model, default: 0; P70=Side knife model, default: 2)

	P-47
	Number of pieces completed
	0-9999
	0
	

	P-48
	Needle goes up as power on
	0-1
	0
	0: OFF
1: ON

	P-50
	Upper positioning adjustment
	0-1439
	
	Same as P-72.

	P-51
	Lower positioning adjustment
	0-1439
	
	Same as P-73.

	P-52
	Testing speed (r/m)
	100-6000
	5500
	

	P-53
	Testing working time
(×100ms)
	1-250
	50
	

	P-54
	Testing stopping time
(×100ms)
	1-250
	20
	

	P-55
	Item A testing: Continuous running
	0-1
	0
	0: OFF
1: ON

	P-56
	Item B testing: With function running
	0-1
	0
	0: OFF
1: ON

	P-57
	Item C testing: Start stop operation
	0-1
	0
	0: OFF
1: ON

	P-58
	Machine plate protection switch
	0-1
	0
	0: OFF
1: ON

	P-59
	[bookmark: OLE_LINK215]Presser foot protection switch
	0-1
	1
	0: OFF
1: ON

	P-60
	Electric /Air-powered
	0-1
	0
	0: Electric
1: Air-powered

	P-61
	Trimming switch by heeling pedal
	0-7
	0
	0: OFF
1: In manual mode
2: In semi-automation
3: In automation
4: In manual mode and semi-automation 
5: In semi-automation and automation
6: In manual mode and automation 
7: ON

	P-63
	Language
	0-2
	1
	0: English
1: Chinese
2: Turkish

	P-64
	[bookmark: OLE_LINK24]The strength of front sensor
	0%-100%
	80%
	[bookmark: OLE_LINK25]Adjustment front sensor strength.

	P-65
	The strength of middle sensor
	0%-100%
	80%
	Adjustment middle sensor strength.

	P-66
	The strength of back sensor
	0%-100%
	80%
	Adjustment back sensor strength.

	P-67
	The sensitivity of back sensor
	0-700
	375
	In order to adapt different cloth material setting back-sensor receive strength.

	P-69
	Response time of back sensor (ms)
	0-3000
	0
	[bookmark: OLE_LINK126][bookmark: OLE_LINK127][bookmark: OLE_LINK128][bookmark: OLE_LINK129]Response time of back-sensor, when sewing such as mesh cloth can adjust this item, then can achieve you want effects.

	Advanced parameter (press [P]+[S] keys at the same time to enter)

	P-70
	Model selection
	1-3
	1
	1: Horizontal knife type
2: Side knife type
3: Thread tip overlocked

	P-71
	Maximum speed limit (r/m)
	200-7000
	6000
	

	P-72
	Manually upper positioning adjustment
	0-2399
	
	Through hand-wheel direction, clockwise turn hand-wheel to up position press [image: ] to save the current value.

	P-73
	Manually lower positioning adjustment
	0-2399
	
	Through hand-wheel direction, clockwise turn hand-wheel to down position then press [image: ] to save current value.

	P-74
	Parameter reference
	N1-N5
	N1
	N1: Control box software version
N2: Panel software version
N3: Rotation
N4: Pedal AD
N5: Driver software version

	P-76
	Password setting
	0-9999
	
	

	P-77
	Zero-point angle setting
	0-1440
	520
	Enter this item and press [image: ] to automatically find the change point, wait for the machine to stop, and press [image: ] to save.

	P-78
	Suction bucket type
	0-2
	1
	0: With brush
1: Without brush
2: Valve

	P-79
	One-click testing
	0-1
	0
	0: OFF
1: ON

	P-80
	The needle bar shield protection switch
	0-1
	0
	0: OFF
1: ON

	P-81
	Electromagnet protection
	0-1
	1
	0: OFF
1: ON

	P-82
	Number of alarms
	0-9990
	0
	

	P-83
	The number of standby display pieces
	0-1
	0
	0: OFF
1: ON

	P-84
	Piece counting mode selection
	0-1
	0
	0: Ascending
1: Descending

	P-85
	Piece counting trimming times
	0-50
	1
	

	P-86
	Voice volume
	0-5
	4
	

	P-87
	Voice broadcast selection
	0-3
	3
	0: OFF
1: Start-up voice only
2: Key tone only
3: ON

	P-88
	User model
	
	0
	

	P-90
	Voice chip selection
	0-4
	4
	

	P-91
	Back sensor switch
	0-1
	1
	0: OFF
1: ON
After the back sensor is turned off, the back sensor is based on the parameter value set in P28.

	P-92
	Start-up language selection
	0-11
	0
	

	P-93
	Lock screen time (s)
	0-300
	10
	

	P-94
	Thin material light transmission
	1-800
	45
	The smaller the number, the stronger the sensitivity, and the larger the number, the weaker the sensitivity.

	P-95
	Ordinary material light transmission
	1-800
	250
	The smaller the number, the stronger the sensitivity, and the larger the number, the weaker the sensitivity.

	P-96
	Grid material light transmission
	1-800
	50
	The smaller the number, the stronger the sensitivity, and the larger the number, the weaker the sensitivity.

	P-97
	Number of special material detection needles
	0-50 (stitches)
	0
	The larger the grid, the greater the number of needles that need to be tested.

	P-98
	Trimming speed switch
	0-3
	0
	0: OFF
1: Front trimming
2: Back trimming
3: ON

	P-99
	Front trimming protection
	0-1
	1
	0: OFF
1: ON

	P-100
	Sewing fabric type
	0-2
	0
	0: Thin material
1: Ordinary material
2: Grid material

	P-101
	Front sensor identification signal difference
	0-50
	10
	

	P-102
	Middle sensor identification signal difference
	0-50
	10
	

	P-103
	Back sensor identification signal difference
	0-50
	10
	

	P-104
	Pedal acceleration slope
	0-4
	2
	The higher the number, the faster the pedal response.

	P-105
	Speed ratio
	0-100
	33
	The higher the number, the higher the rotation speed (real number).

	P-106
	Back pedal trimming times
	0-1
	0
	0: Trimming once when back pedal after sewing is completed;
1: Trimming every time when back pedal after sewing is completed.
(Use with P-61)

	P-110
	Sensor fast-reading calibration at power-up
	0-1
	1
	0: OFF
1: ON

	P-111
	High speed switch
	0-1
	0
	0: OFF
1: ON

	P-112
	Back thread trimming mode
	0-1
	0
	0: OFF
1: ON

	P-113
	Short thread residue mode
	0-1
	0
	0: OFF
1: ON

	P-114
	Number of front short thread residue stitches
	0-50
	22
	

	P-115
	Number of back short thread residue stitches
	0-50
	0
	

	P-129
	Stepping motor switch
	0-1
	1
	0: OFF
1: ON

	P-130
	Stepping motor original point
	-2400~2400
	0000
	Need to lock the P131 stepping motor off.

	P-131
	Stepping motor lock
	0-1
	0
	0: Locked
1: Release

	P-132
	Maximum current of stepping motor
	20-60
	50
	(*100mA) The maximum current when the stepping motor is running.

	P-133
	Steady current of stepping motor
	5-30
	20
	(*100mA) The steady current of stepping motor when the presser foot is raised (that is the steady force of the presser foot).

	P-134
	Stepping motor speed when switch from controlling feed dog to controlling thread trimming
	5-1500
	1200
	

	P-135
	Starting angle of thread trimming
	-2400~2400
	370
	

	P-136
	Thread trimming speed
	5-1500
	400
	

	P-137
	Thread trimming angle
	0-730
	150
	

	P-138
	Thread trimming return speed
	5-1500
	200
	

	P-139
	Stepping motor speed for returning to origin
	5-1500
	200
	

	P-140
	Stepping motor speed when switch from controlling thread trimming to controlling feed dog
	5-1500
	700
	

	P-141
	Presser foot 10th gear angle
	-2400~2400
	420
	

	P-142
	Presser foot lifting speed
	5-1500
	600
	

	P-143
	Maximum limiting angle of presser foot
	400-700
	590
	

	P-144
	Presser foot lowering speed
	-5~1500
	300
	

	P-149
	Feed dog height of thin fabric
	0-300
	200
	

	P-150
	Feed dog height of medium thick fabric
	0-300
	125
	

	P-151
	Feed dog height of thick fabric
	0-300
	0
	

	P-152
	Transparency of transparent material
	1-800
	45
	

	P-153
	Timing fine-tuning of front trimming
	0-100
	10
	

	P-154
	Locking current of stepping motor at the origin
	1-12
	4
	

	P-155
	Holding time for stepping motor debugging
	0-300
	10
	

	P-162
	Number of back presser foot micro-lifting delayed stitches
	0-100
	3
	

	P-163
	Back presser foot micro-lifting lowering timing
	0-50
	10
	

	P-164
	Presser foot micro-lifting switch
	0-3
	1
	0: OFF
1: Front presser foot
2: Back presser foot
3: ON

	P-165
	The detection stitches number of presser foot micro-lifting
	0-50
	2
	

	P-166
	Presser foot micro-lifting angle
	0-600
	200
	

	P-167
	Presser foot micro-lifting speed
	5-1500
	100
	

	P-168
	Presser foot micro-lifting lowering speed
	5-1500
	150
	

	P-169
	Fabric mode
	0-4
	0
	0: Knitted T-shirt
1: Denim
2: Jacket and pants
3: Elastic fabric
4: Non-woven fabric

	P-170
	Maximum speed of knitted T-shirt
	200-7000
	5500
	Item P01 shall prevail.

	P-171
	Feed dog height of knitted T-shirt
	0-2
	1
	Corresponds to P149-151.
0: Thin fabric
1: Medium thick fabric
2: Thick fabric

	P-174
	Presser foot height of knitted T-shirt
	1-15
	15
	

	P-175
	Maximum speed of denim
	200-7000
	5500
	Item P01 shall prevail.

	P-176
	Feed dog height of denim
	0-2
	2
	Corresponds to P149-151.
0: Thin fabric
1: Medium thick fabric
2: Thick fabric

	P-179
	Presser foot height of denim
	1-15
	12
	

	P-180
	Maximum speed of jacket and pants
	200-7000
	5500
	Item P01 shall prevail.

	P-181
	Feed dog height of jacket and pants
	0-2
	1
	Corresponds to P149-151.
0: Thin fabric
1: Medium thick fabric
2: Thick fabric

	P-184
	Presser foot height of jacket and pants
	1-15
	10
	

	P-185
	Maximum speed of elastic fabric
	200-7000
	5500
	Item P01 shall prevail.

	P-186
	Feed dog height of elastic fabric
	0-2
	0
	Corresponds to P149-151.
0: Thin fabric
1: Medium thick fabric
2: Thick fabric

	P-189
	Presser foot height of elastic fabric
	1-15
	6
	

	P-190
	Maximum speed of non-woven fabric
	200-7000
	5500
	Item P01 shall prevail.

	P-191
	Feed dog height of non-woven fabric
	0-2
	0
	Corresponds to P149-151.
0: Thin fabric
1: Medium thick fabric
2: Thick fabric

	P-194
	Presser foot height of non-woven fabric
	1-15
	6
	

	P-195
	Translucency of knitted T-shirt
	0-3
	0
	

	P-196
	Translucency of denim
	0-3
	0
	

	P-197
	Translucency of jacket and pants
	0-3
	0
	

	P-198
	Translucency of elastic fabric
	0-3
	0
	

	P-199
	Translucency of non-woven fabric
	0-3
	0
	


Note: the initial value of parameters is for reference only, and the actual value of parameters is subject to the real object.

4. Error code list
	Error code
	Problem
	Solution

	E01
	System overvoltage
	Please cut off the power supply and confirm whether the power supply voltage is correct (or whether it exceeds the rated voltage specified for use).

	E02
	System undervoltage
	Please cut off the power supply and confirm whether the power supply voltage is correct (or is it lower than the rated voltage specified for use).

	E05
	Speed controller failure
	Please cut off the power and confirm whether the speed controller is correctly connected to the control box.

	E07
	Motor locked-rotor
	Please turn the handwheel to confirm whether main shaft motor is locked. Turn the handwheel 45° after the alarm can automatically eliminate the alarm.
Please confirm whether the encoder cable or the motor and the power cable of the motor are properly connected.

	E11
	Unable to find the upper position
	Please cut off the power supply, check whether the connection of the positioning signal board on the control box is loose, or whether the handwheel installation location is standardized, restore it to normal and restart the system.

	E14
	Encoder signal is abnormal
	Please cut off the power, check whether the motor encoder connector is loose or fall off, restore it to normal and restart the system.

	E15
	System overcurrent protection
	Please cut off the power, check whether the motor power supply cable is damaged or abnormally connected, and restart after troubleshooting.

	E16
	Incorrect position of presser foot
	Check whether the presser foot is open, whether the presser foot safety switch is damaged, and whether the socket is abnormal.

	E17
	Incorrect position of sewing table
	Check whether the sewing table is open, whether the safety switch of the sewing table is damaged, and whether the socket is abnormal.

	E92
	Thread trimming (presser foot) stepping motor overcurrent
	Turn off the system power and observe whether the thread trimming (presser foot) stepping motor is stuck. If it is stuck, remove the mechanical failure of the machine head first. If it is normal, check if the thread trimmer (presser foot) stepping motor interface is loose or fall off, restore it to normal and restart the system.

	E94
	Thread trimming (presser foot) stepping motor can’t find zero-point
	Turn off the system power and observe whether the thread trimming (presser foot) stepping motor is stuck. If it is stuck, remove the mechanical failure of the machine head first. If it is normal, check whether the thread trimming (presser foot) stepping motor encoder interface is loose or falling off, and whether there is oil on the encoder code disk. If there is any oil, please clean it up, restore it to normal and restart the system.

	E95
	Thread trimming (presser foot) stepping motor encoder signal is abnormal
	Turn off the system power, check if the thread trimming (presser foot) stepping motor encoder interface is loose or fall off, restore it to normal and restart the system.

	E96
	Thread trimming (presser foot) stepping motor is not connected
	Turn off the power of the system, check whether the wire trimming (presser foot) stepping motor power cord interface and encoder interface are loose or fall off, and restart the system after returning it to normal.

	E97
	Thread trimming (presser foot) stepping motor stalling
	Turn off the system power and observe whether the thread trimming (presser foot) stepping motor is stuck. If it is stuck, remove the mechanical failure of the machine head first. If it is normal, check whether the wire trimming (presser foot) stepping motor power cord interface and encoder interface are loose or fall off, restore them to normal and restart the system.

	NC
	Abnormal communication
	Turn off the system power and check whether the panel connector is loose or disconnected. After troubleshooting, if the fault persists, check whether the power supply indicator of the main control chip is on. If abnormal, please replace the control box.



5. Port diagram
8P white port (LED, launcher)
[image: ]
1: LED-, 2: +5V, 3: Manual trimming, 4: GND, 5: Middle launcher, 6: Back launcher, 7: Front Launcher, 8: +5V

3P black port (presser foot position sensing)
[image: ]
1: GND, 2: signal, 3: +5V

3P red port (sewing table position sensing)
[image: ]
1: GND, 2: signal, 3: +5V

2P black port (front receiving)
[image: ]
1: Received signal, 2: +5V

2P red port (medium receiving)
[image: ]
1: Received signal, 2: +5V

2P white port (back receiving)
[image: ]
1: Received signal, 2: +5V

6P white port (suction)
[image: ]
1. Thread chain suction: 1, 4 (+24V)
2. Cloth suction: 2, 5 (+24V)
3. Thread tension releasing: 3, 6 (+24V)


6

image5.png




image6.png




image7.png
<

Cloth Choice





image8.png




image9.png




image10.png




image11.png




image12.png




image13.png




image14.png
—RIRR

Switching





image15.png
<

Cloth Choice




image16.png




image17.png




image18.png




image19.png




image20.png




image21.png




image22.png




image23.png




image24.png




image25.png




image26.png




image27.png




image28.png




image29.png




image30.emf

image2.wmf

image3.png




image4.png




