[bookmark: OLE_LINK146][image: MCj03463170000[1]]Safety Instruction
1. [bookmark: OLE_LINK149]Users are required to read the operation manual completely and carefully before installation or operation.
2. [bookmark: OLE_LINK152][bookmark: OLE_LINK153]The product should be installed and pre-operated by well-trained persons. All power supplies must be turned off during the installation work, remember not to operate with power on. 
3. All the instruction marked with sign [image: MCj03463170000[1]] must be observed or executed. Otherwise, bodily injuries might occur.
4. [bookmark: OLE_LINK154][bookmark: OLE_LINK155]For perfect operation and safety, it is prohibited that using extension cable with multi-outlet for power connection. 
5. [bookmark: OLE_LINK156]When connecting the power cord, it must be determined that the operating voltage conforms to the rated voltage value specified in the product identification.
6. [bookmark: OLE_LINK166]Don＇t operate in direct sun light，outdoors area and where the room temperature is over 45°C or below 0°C.
7. [bookmark: OLE_LINK167][bookmark: OLE_LINK168]Please avoid operating near the heater at dew area or at the humidity below 10% or above 90%.
8. [bookmark: OLE_LINK169]Don＇t operate in area with heavy dust, corrosive substance or volatile gas.
9. [bookmark: OLE_LINK170][bookmark: OLE_LINK171]Avoid power cord being applied by heavy objects or excessive force, or over bend.
10. [bookmark: OLE_LINK172][bookmark: OLE_LINK173]The earth wire of power cord must be connected to the system ground of the production plant by proper size of conductions and terminals. This connection should be fixed permanently.
11. [bookmark: OLE_LINK174][bookmark: OLE_LINK175]All the moving portions must be prevented to be exposed by the parts provided.
12. [bookmark: OLE_LINK176]Turing on the machine in the first time, operate the sewing machine at low speed and check the correct rotation direction.
13. [bookmark: OLE_LINK177][bookmark: OLE_LINK178]Turn off the power before the following operation: 
[bookmark: OLE_LINK179][bookmark: OLE_LINK180]1. Connecting or disconnecting any connectors on the control box or motor.
[bookmark: OLE_LINK181][bookmark: OLE_LINK182]2. Threading needle.
[bookmark: OLE_LINK183][bookmark: OLE_LINK184]3. Raising the machine head.
[bookmark: OLE_LINK185][bookmark: OLE_LINK186]4. Repairing or doing any mechanical adjustment.
[bookmark: OLE_LINK187][bookmark: OLE_LINK188]5. Machines idling.
14. [bookmark: OLE_LINK189]Repairs and high level maintenance work should only be carried out by electronic technicians with appropriate training.
15. [bookmark: OLE_LINK190][bookmark: OLE_LINK191]All the spare parts for repair must be provided or approved by the manufacturer.
16. [bookmark: OLE_LINK192][bookmark: OLE_LINK193]Don’t use any objects or force to hit or ram the product.
Guarantee Time
Warranty period of this product is 1 year dated from purchasing, or within 2 years from ex-factory date.
Warranty Detail
Any trouble found within warranty period under normal operation, it will be repaired free of charge. However, maintenance cost will be charged in the following cases even if within warranty period:
[bookmark: OLE_LINK102][bookmark: OLE_LINK103]1. Inappropriate use, including: wrong connecting high voltage, wrong application, disassemble, repair, modification by incompetent personnel, or operation without the precaution, or operation out of its specification range, or inserting other objects or liquids into the product.
2. Damage by fire, Earth quake, lighting, wind, flood, salt corrosive, moisture, abnormal power voltage and any other damage cause by the natural disaster or by the inappropriate environments.
3. Dropping after purchasing or damage in transportation by customer himself or by customer’s shipping agency
* We make our best effort to test and manufacture the product for assuring the quality. However, it is possible that this product can be damaged due to external magnetic interference and electronic static or noise or unstable power source more than expected. Therefore the grounding system of operate area must guarantee the good earth and it’s also recommended to install a failsafe device (Such as residual current breaker).



1 Button displays and operating instructions
1.1 Key description
	Name
	key
	Indicate

	Function key
	
	If press, enter or exit function parameter edit mode.
If long-press, switch to the password input interface. Enter the correct password, press the S key to confirm, you can enter the advanced parameter setting interface.

	Enter key
	
	For the content of the selected parameters check and save: after select parameter press this key to check and modify operation, after modified parameter value press this key to exit and save the parameter.
In the main interface, if long-press, switch to the debugging parameter interface. P72, P92, P100 can be adjusted.

	Left selection
	
	The parameter bit is shifted left.

	Right selection
	
	The parameter bit is shifted right.

	Parameter increasing
	
	If press, the parameter will be increased.
If long-press, the parameter will be increased continuously.

	Parameter decreasing
	
	If press, the parameter will be decreased.
If long-press, the parameter will be decreased continuously.

	Speed increasing
	
	If press, the speed will be increased.

	Speed decreasing
	
	If press, the speed will be decreased.

	LED brightness adjustment
	
	In the main interface, if press, adjust LED brightness.

	Soft start setting
	
	In the main interface, if press, set used or cancelled soft start function.

	Presser foot lifting setting
	
	In the main interface, if press, set used or cancelled presser foot lifting function.

	Needle stopping position selection
	
	In the main interface, if press, switch between upper and lower needle stop positions.




1.2 Auxiliary function
1.2.1 Debugging mode
Long press “[image: ]” in the main interface, switch to the debugging parameter interface. P72, P92, P100 can be adjusted.

2 User parameter
	No.
	Items
	Range
	Default
	Description

	P01
	Maximum sewing speed (rpm)
	100-9000
	5000
	

	P02
	Acceleration curve adjustment (%)
	10-100
	80
	

	P03
	Needle stopping position selection
	UP/DN
	UP
	UP: Upper stopping position
DN: Lower stopping position

	P04
	Output duty cycle of upper thread wiping electromagnet
	0-100
	75
	

	P05
	Upper thread wiping action time (ms)
	10-990
	20
	

	P06
	Upper thread wiping return time (ms)
	10-990
	15
	

	P07
	Soft start speed (rpm)
	200-1500
	1000
	

	P08
	The number of stitches for soft start (stitch)
	0-99 
	2
	

	P14
	Soft start function selection
	ON/OFF
	OFF
	

	P15
	LED brightness setting
	0-4
	3
	

	P21
	The position of the pedal for accelerating
	30-1000
	500
	

	P22
	The position of the pedal for the stop
	30-1000
	420
	

	P23
	The position of the pedal for presser foot lifting
	30-1000
	280
	

	P24
	The position of the pedal for thread trimming
	30-1000
	130
	

	P29
	The stopping force when thread trimming
	1-45
	20
	

	P37
	Thread trimming of upper knife output function setting
	0-11
	1
	

	P39
	Automatic presser foot lifting when pause
	UP/DN
	DN
	UP: ON
DN: OFF

	P40
	Automatic presser foot lifting after trimming
	UP/DN
	DN
	UP: ON
DN: OFF

	P41
	Counter display
	0-9999
	
	Display the quantity of finished sewing piece. Long-press “-” key to clear the count.

	P42-N01
	Main software version
	
	
	

	P42-N02
	Panel software version
	
	
	

	P42-N03
	Speed
	
	
	

	P42-N04
	The pedal AD
	
	
	

	P42-N05
	The mechanical angle (upper position)
	
	
	

	P42-N06
	[bookmark: _GoBack]The mechanical angle (lower position)
	
	
	

	P42-N07
	Busbar voltage AD
	
	
	

	P42-N25
	View virtual password
	
	
	

	P43
	Direction of motor rotation
	CCW/CW
	CW
	CW: Clockwise
CCW: Counter clockwise

	P44
	Normal stopping force
	1-45
	15
	

	P48
	The minimum speed (positioning speed) (rpm)
	200-1000
	500
	Adjust the minimum speed.

	P50
	Presser foot full output time
	10-990
	150
	

	P51
	Cycle signal of presser foot output
	1-80
	30
	

	P52
	Delay the start of the motor to protect the lowering time of presser foot (ms)
	10-990
	100
	Delay the start time, with automatic presser foot down.

	P53
	Presser foot lifting function selection
	0-2
	1
	0: OFF
1: Back pedaling and half back pedaling with lifting presser foot
2: Half back pedaling without lifting presser foot, back pedaling with lifting presser foot

	P54
	Thread trimming of lower knife action time
	0-100
	10
	

	P55
	Thread trimming of upper knife action time (ms)
	10-990
	20
	

	P56
	Power on and positioning
	0-2
	0
	0: Always not to find the upper position
1: Always to find the upper position
2: If the motor is already in the upper position, no longer find the upper position

	P57
	Presser foot protection time (s)
	1-120
	10
	Forced to close after lifting the presser foot for a holding time.

	P58
	Upper positioning adjustment
	0-2399
	
	Upper positioning adjustment, the needle will advance stop when the value decreased, the needle will delay stop when the value increased.

	P59
	Down positioning adjustment
	0-2399
	
	Down positioning adjustment, the needle will advance stop when the value decreased, the needle will delay stop when the value increased.

	P60
	Testing speed (rpm)
	100-5500
	4000
	Setting testing speed.

	P61
	Testing A
	ON/OFF
	OFF
	Continuous running testing.

	P62
	Testing B 
	ON/OFF
	OFF
	Start and stop testing with all functions.

	P63
	Testing C
	ON/OFF
	OFF
	Start and stop testing without all function.

	P64
	Test running time
	1-250
	50
	

	P65
	Test stopping time
	1-250
	50
	

	P67
	Lower thread trimming position protection switch
	ON/OFF
	ON
	

	P68
	Maximum speed limit (rpm)
	100-5500
	5500
	

	P69
	Motor type selection
	0-50
	0
	

	P70
	Model selection
	1-45
	32
	

	P71
	Presser foot lowering buffer duty cycle (%)
	0-50
	0
	

	P72
	Quick adjustment of upper positioning
	0-2399
	
	Adjust up needle position, the displayed value will change with the position of the handwheel, press "S" key to save the current position (value) as up needle position.

	P73
	Quick adjustment of down positioning
	0-2399
	
	Adjust down needle position, the displayed value will change with the position of the handwheel, press "S" key to save the current position (value) as down needle position.

	P86
	Upper and lower positioning distance
	0-2399
	1200
	

	P87
	The delayed return time for thread trimming of upper knife (ms)
	10-990
	15
	

	P89
	AC overvoltage setting
	500-1023
	880
	

	P92
	Electrical angle correction of motor
	
	160
	Reading the initial Angle of encoder, the factory default was set, please do not change the values (parameter value cannot be changed manually, random change it will result the control box and motor abnormal or damaged).

	P93
	The delayed time of half back pedaling (ms)
	10-900
	150
	

	P104
	Password setting
	0000-9999
	2016
	

	P108
	Suction function selection
	0-1
	0
	0: OFF
1: ON

	P113
	Presser foot lifting holding phase control type
	0-1
	0
	0: Open loop
1: Closed loop

	P116
	The working time of press foot lowering buffer (ms)
	0-990
	30
	

	P117
	The delayed time of press foot lowering buffer (ms)
	0-990
	20
	

	P119
	Electromagnet overcurrent protection
	0-1
	1
	0: No alarm, turn off the output.
1: Alarm and shutdown.


Note: the initial value of parameters is for reference only, and the actual value of parameters is subject to the real object.

3 Error code list
	Error code
	Problem description 
	Solutions

	E01
	High voltage
	1. Whether the grid voltage is higher than AC260V.
2. If it is self-generated power supply, please reduce the generator power.
3. If it still does not work normally, please replace the control box and notify the after-sales service.

	E02
	Low voltage
	1. Whether to connect to low voltage.
2. Reset.
3. If it still does not work normally, please replace the control box and notify the after-sales service.

	E03
	CPU communication abnormal
	1. Turn off the system power and check whether the connection of the display screen is loose or disconnected, restart the system after returning it to normal.
2. Turn off the system power, remove the control box and only plug in the power cord to power on, whether alarm E03, if it still alarms E03, replace the control box and notify the after-sales service.

	E05
	Pedal signal abnormal
	1. Check whether the pedal connector is loose or fall off, and restart the system after returning it to normal.
2. If it still does not work normally, please replace the control box or speed controller and notify the after-sales service.

	E07
	Main shaft motor locked-rotor
	1. Turn off the power and check whether the handwheel can be turned smoothly (turn the handwheel by hand), if it cannot be turned, please check the machine.
2. Turn off the power, check whether the motor power connector is loose, plug it in and restart it.
3. Check whether the upper needle stop position is correct, if not, please adjust the upper positioning position.
4. If it still does not work normally, please replace the control box or spindle motor and notify the after-sales service.

	E10
	Electromagnet overcurrent protection
	Turn off the system power and check the solenoid (solenoid valve) for damage or short circuit.

	E09
E11
	The positioning signal of main shaft motor encoder is abnormal
	1. Turn off the system power, check whether main shaft motor encoder connector is loose or fall off, restore it to normal and restart the system.
2. Check whether the motor zero point correction setting is correct; Reset the motor zero point correction; Whether there is oil on the encoder code plate, please clean it if there is any.
3. If it still does not work normally, please replace the control box or main shaft motor and notify the after-sales service.

	E14
	Main shaft motor encoder signal is abnormal
	1. Turn off the system power, check whether the main shaft motor encoder connector is loose or fall off, restore it to normal and restart the system.
2. Check whether the grating is installed correctly (whether the grating screws are tightened and whether the grating is in the center of the encoder).
3. Check whether there is oil on the encoder code plate, if there is, please clean it up, and restart the system after recovery.
4. If it still does not work normally, please replace the control box or main shaft motor and notify the after-sales service.

	E15
	Main shaft motor drive overcurrent
	1. Please check whether the motor power cord has bad contact.
2. Please check whether the motor power cord is crushed.
3. Please replace the control box or main shaft motor and notify the after-sales service.

	E20
	Main shaft motor failed to start
	1. Turn off the system power, check whether main shaft motor power cord connector and encoder connector are loose or fall off, restore them to normal and restart the system.
2. Check whether the motor zero point correction setting is correct, reset the motor zero point correction.
3. If it still does not work normally, please replace the control box or main shaft motor and notify the after-sales service.

	E94
	The positioning signal of trimming (presser foot) stepping motor encoder is abnormal
	1. Turn off the system power and observe whether trimming (presser foot) stepping motor is stuck. If it is stuck, remove the mechanical failure of the machine first. If it is normal, check whether trimming (presser foot) stepping motor encoder connector is loose or falling off, and whether there is oil on the encoder code plate. If there is, please clean it up, restore it to normal and restart the system.
2. If it still does not work normally, please replace the control box or trimming (presser foot) stepping motor and notify the after-sales service.

	E95
	Trimming (presser foot) stepping motor encoder signal is abnormal
	1. Turn off the system power, check if the thread trimming (presser foot) stepping motor encoder connector is loose or fall off, restore it to normal and restart the system.
2. If it still does not work normally, please replace the control box or the thread trimming (presser foot) stepping motor and notify the after-sales service.

	E96
	Trimming (presser foot) stepping motor failed to start
	1. Turn off the power of the system, check whether the thread trimming (presser foot) stepping motor power cord connector and encoder connector are loose or fall off, and restart the system after returning it to normal.
2. If it still does not work normally, please replace the control box or the thread trimming (presser foot) stepping motor and notify the after-sales service.

	E98
	The stepping motor is locked-rotor when presser foot lifting
	1. Turn off the system power and observe whether the thread trimming (presser foot) stepping motor is stuck. If it is stuck, remove the mechanical failure of the machine first. If it is normal, check whether the thread trimming (presser foot) stepping motor power cord connector and encoder connector are loose or fall off, restore them to normal and restart the system.
2. If it still does not work normally, please replace the control box or the thread trimming (presser foot) stepping motor and notify the after-sales service.

	E99
	The stepping motor overcurrent when presser foot lifting
	1. Turn off the system power and observe whether the thread trimming (presser foot) stepping motor is stuck. If it is stuck, remove the mechanical failure of the machine first. If it is normal, check whether the thread trimming (presser foot) stepping motor power cord connector and encoder connector are loose or fall off, restore them to normal and restart the system.
2. If it still does not work normally, please replace the control box or the thread trimming (presser foot) stepping motor and notify the after-sales service.



4 Port diagram
2P function port description
[image: ]
	1. LED lights: 1 (DGND), 2 (+5V)
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